

**C/E 3904 – Dual Master Cylinder Mount**

**Parts List:**

1…Master Cylinder Mount Plate 2…Mount Plate Gussets

These instructions are just one way of properly installing the Dual Master Cylinder Mount. Depending on your fabrication experience, you may find it easier or more convenient using other methods that accomplish the same results. Every installation is slightly different, and we have attempted to structure these instructions to make your installation as easy as possible.

1…Find the best location for the master cylinder on the floor frame rail. The mount location needs to clear of the heat from the headers. Make sure the caps and brakes lines are easily accessible. Mount the master cylinder before you place the brake pedal.

2…Bolt the master cylinder to the plate. Hold the assembly in the predetermined location. Make sure that the brake rod when installed will be in line with the brake pedal when it is installed. There should be no obstructions to this alignment. Double check that there is ample ground clearance.

3…Tack weld the bracket into place on the chassis. Tack weld one gusset to the plate and the chassis. The top gusset will be towards the front of the car and bottom gusset towards the rear.

4…Remove the master cylinder and final weld the bracket and gussets to the chassis.

A drawing of a square object

AI-generated content may be incorrect.